# WWW server root
Sys.Dir.WWW="SF:0:\www"
#Sys.Dir.WWW="SD:0:\www"
# Hostname
Net.Dev.1.Name="NPD_DSC_CarDV"
# Set WiFi as a station mode
# Net.Dev.1.Type="STA"
# Set WiFi as a AP mode
Net.Dev.1.Type="AP"
#
# In STATION mode, Net.Dev.1.BootProto could be DHCP or STATIC.
# In AP mode, Net.Dev.1.IPV4.Address and Gateway must be set
Net.Dev.1.BootProto="DHCP"
Net.Dev.1.IPV4.Address="192.72.1.1"
Net.Dev.1.IPV4.Gateway="192.72.1.1"
#
# Service ports for RTSP, HTTP, HTTPS
Net.Port.Service="554, 80, 80"
#
# for AP mode
Net.WIFI_AP.SSID="NPD_CarDV_WiFi_lei"
Net.WIFI_AP.EncType="AES"
Net.WIFI_AP.CryptoKey="1234567890"
#
# Secondary AP for Remote
#
Net.WIFI_AP1.SSID="RC_NPD_CarDV-actioncamera"
Net.WIFI_AP1.EncType="AES"
Net.WIFI_AP1.CryptoKey="1234567890"
Net.WIFI_AP1.HideSSID=YES
#
# for STATION mode
# Try to connect to an AP as follow ordering
# EncType could be AES or TKIP, AES is for WPA2-PSK, TKIP is for WPA-PSK
Net.WIFI_STA.AP.2.SSID="YourAP1"
Net.WIFI_STA.AP.2.EncType="AES"
Net.WIFI_STA.AP.2.CryptoKey="1234567890"
#
Net.WIFI_STA.AP.3.SSID="YourAP2"
Net.WIFI_STA.AP.3.EncType="AES"
Net.WIFI_STA.AP.3.CryptoKey="1234567890"
#
Net.WIFI_STA.AP.4.SSID="YourAP3"
Net.WIFI_STA.AP.4.EncType="TKIP"
Net.WIFI_STA.AP.4.CryptoKey="1234567890"
#
Net.WIFI_STA.AP.5.SSID="Coke"
Net.WIFI_STA.AP.5.EncType="AES"
Net.WIFI_STA.AP.5.CryptoKey="helloworld"
#
Net.WIFI_STA.AP.6.SSID="ZyXAIT99"
Net.WIFI_STA.AP.6.EncType="AES"
Net.WIFI_STA.AP.6.CryptoKey="1234567890"
# MJPEG Streaming
Camera.Preview.MJPEG.bitrate=4000000
Camera.Preview.MJPEG.w=320
Camera.Preview.MJPEG.h=240
Camera.Preview.MJPEG.fps=30
#
# 1 Enable liveRTSP/av1 for Audio and Video live streaming
# 2 Enable liveRTSP/v1
Camera.Preview.H264.w=1280
Camera.Preview.H264.h=720
Camera.Preview.H264.bitrate=4000000
Camera.Preview.RTSP.rtcp=0
#1: MJPG, 4:H264
Camera.Preview.RTSP.av=4  
Camera.Preview.RTSP.keepalive=60
#
